**Appendix A**. Imaging parameters for standard breast MRI protocol.

|  |  |
| --- | --- |
| Coil | Sense breast 16-channel |
| Matrix | 400 x 400 |
| Pixel spacing (mm) | 0.8542 |
| Field of View (mm) | 3422 |
| In-plane resolution (mm) | 0.92 |
| Repetition time (msec) | 2000 |
| Echo time (msec) | 218 |
| Flip angle (°) | 90 |
| Echo train length | 95 |
| Slice thickness (mm) | 2.0 |