**Magnetic Assembly Route to Construct Reproducible and Recyclable SERS Substrate**

*Bingfang Zou*a,b*, Chunyu Niu*a*, Ming Ma*a*, Lu Zhao*a*, Yongqiang Wang*a∗

a Key Laboratory for Special Functional Materials of the Ministry of Education, Henan University, Kaifeng 475004, P. R. China

b School of Physics and Electronics, Henan University, Kaifeng 475004, P. R. China.

∗Corresponding author. Email: wangyq@henu.edu.cn

****

**Figure S1.** The Fe3O4@SiO2@TiO2 composite microspheres synthesized without using ultrasonic.



**Figure S2.** The Fe3O4@SiO2@TiO2 composite microspheres synthesized without using mechanical stirrer.

****

**Figure S3.** A calibration curve where the logarithmic intensity measured at 1363 cm−1 peak is plotted versus the logarithmic concentration of R6G. Error bars are standard deviations calculated from 20 independent measurements.