**Three Dimensional CuO/TiO2 Hybrid Nanorod Arrays Prepared by Electrodeposition in AAO Membranes as an Excellent Fenton-like Photocatalyst for Dye Degradation**

Manisha Kondiba Date1,2, 3, Li-Heng Yang1,2, 3, Tzu-Yi Yang1,2, 3, Kuang-ye Wang1,2, 3, Teng-Yu Su1,2, 3, Ding-Chou Wu1,2, 3, Yu-Lun Cheuh1,2, 3\*

*1Department of Materials Science and Engineering& Frontier Research Center on Fundamental and Applied Sciences of Matters National Tsing Hua University, Hsinchu 30013, Taiwan*

*2Department of Physics, National Sun Yat-Sen University, Kaohsiung, 80424, Taiwan*

*3Frontier Research Center on Fundamental and Applied Sciences of Matters, National Tsing Hua University, Hsinchu 30013, Taiwan.*

\*Corresponding email: ylchueh@mx.nthu.edu.tw



**Figure S1.** Cross-section SEM image of 6.53 µm long CuO NRs in AAO (scale bar: 1 µm).



**Figure S2**. XRD spectrum of TiO2 capping CuO NRs annealed at 600°C,over the 2θ ranges of 25°-29°.



**Figure S3**. Degradation results of different TiO2 thickness annealed at 500 °C capping 1.85 µm long CuO NR arrays.